SWAPLABEL(8)

NAME
swaplabel - print or change the label or UUID of a swap area

SYNOPSIS
swaplabel [-L label] [-U UUID] device

DESCRIPTION
swaplabel will display or change the label or UUID of a swap partition located on device (or regular file).

If the optional arguments -L and -U are not given, swaplabel will simply display the current swap-area label and UUID of device.

If an optional argument is present, then swaplabel will change the appropriate value on device. These values can also be set during swap creation using mkswap(8). The swaplabel utility allows to change the label or UUID on an actively used swap device.

OPTIONS

-h, --help
    Display help text and exit.

-L, --label label
    Specify a new label for the device. Swap partition labels can be at most 16 characters long. If label is longer than 16 characters, swaplabel will truncate it and print a warning message.

-U, --uuid UUID
    Specify a new UUID for the device. The UUID must be in the standard 8-4-4-4-12 character format, such as is output by uuidgen(1).

AUTHOR
swaplabel was written by Jason Borden <jborden@bluehost.com> and Karel Zak <kzak@redhat.com>.

ENVIRONMENT

LIBBLKID_DEBUG=all
    enables libblkid debug output.

AVAILABILITY
The swaplabel command is part of the util-linux package and is available from https://www.kernel.org/pub/linux/utils/util-linux/.

SEE ALSO
uuidgen(1), mkswap(8), swapon(8)